{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["单位"],"read":"whole","date_system":"1900"}

{"sheet":"单位","index":0,"n_rows":67,"n_cols":7,"rows_kept":67,"merged":[[0,0,0,6],[66,0,66,6]]}
["劳保用品报价清单"]
["序号","名称","规格型号","单位","品牌","价格（元）","备注"]
[1,"安全帽","高强度ABS材质，符合国标","顶"]
[2,"棉安全帽","羊剪绒、ABS材质帽壳、PU面料","顶"]
[3,"面罩安全帽","ABS材质、配有机玻璃面罩","顶"]
[4,"防护头盔","PVC耐酸碱","顶"]
[5,"工作帽","红色、帆布面料、带帽沿、后部可调节","顶"]
[6,"披肩帽","牛仔布900*680mm（±10mm）","个"]
[7,"厨师帽","白色涤棉材质、无檐、头尾60cm带松紧","顶"]
[8,"线手套","纯棉60g/双（±5g）","双"]
[9,"帆布手套","全棉帆布（25cm*14cm）","双"]
[10,"电焊手套","长400mm（±10mm）、天然皮革、耐高温","双"]
[11,"白纱手套","纯棉不起球、耐磨防滑","双"]
[12,"防冻伤手套","长400mm（±10mm）、天然皮革","双"]
[13,"耐酸手套","长400 mm（±10mm）、耐酸碱","双"]
[14,"耐油手套","丁晴胶、全棉针织绒内衬","双"]
[15,"线胶手套","表面浸胶起皱、棉纺织、天然乳胶","双"]
[16,"橡胶手套"," PVC塑胶材质、长320mm（±10mm）","双"]
[17,"12KV绝缘手套","天然橡胶材质、绝缘防水、耐压等级12KV","双"]
[18,"35KV绝缘手套","天然橡胶材质、绝缘防水、耐压等级35KV","双"]
[19,"手扪子","外层两层纱卡布10858，内层3层全棉纱布，中间夹毛毯。","双"]
[20,"全棉手扪子","外层2016全棉布内层全棉包皮布10层","双"]
[21,"耐酸服","耐酸碱，符合国标","套"]
[22,"汽包服","劳动布、连体大号","套"]
[23,"厨师服","全工艺面料，上衣白色、裤子深蓝色","套"]
[24,"一次性防护服","SF透气膜无纺布/连体带帽带脚套/防水防尘防油污","件"]
[25,"劳保鞋","防砸、防穿刺、耐高温、防静电","双"]
[26,"解放鞋","高腰、橡胶底、帆布面料","双"]
[27,"绝缘鞋","帆布面料、绝缘胶底、高腰、耐压等级5KV","双"]
[28,"棉绝缘鞋","棉鞋、帆布面料、绝缘胶底、高腰、耐压等级10KV","双"]
[29,"25KV绝缘靴","天然橡胶材质、绝缘防水、耐压等级25KV","双"]
[30,"35KV绝缘靴","天然橡胶材质、绝缘防水、耐压等级35KV","双"]
[31,"耐油耐酸鞋","牛皮、橡胶底、耐油耐酸碱、棉布内衬","双"]
[32,"耐油皮鞋","牛皮耐油面料、耐磨防滑聚乙酯底","双"]
[33,"防尘口罩","自吸过滤式、防颗粒物","个"]
[34,"防毒口罩","单滤盒活性炭，自吸过滤式","个"]
[35,"纱布口罩","18层全纱布，符合国标","个"]
[36,"3M防毒口罩","上海产3M7502型，含滤盒2个(6003CN)，垫子2个(5N11)，罩子2个(5010）","套"]
[37,"半面罩防毒面具","地球牌（上海跃丰）7100-4/7滤毒盒","套"]
[38,"全面罩防毒面具","防二氧化硫（唐丰牌）","个"]
[41,"配帽面罩","PVC材质、配安全帽用、金属支架","个"]
[42,"有机面罩","非封闭式隔热，带帆布披肩、PVC材质","个"]
[43,"防颗粒物呼吸器","霍尼韦尔H930","个"]
[46,"高效防颗粒呼吸器","保卫康3700","个"]
[47,"高效防颗粒呼吸器滤棉","保卫康3700","片"]
[48,"4#、7#滤毒罐","#7防氯气","个"]
[49,"耳塞","泡棉材质","副"]
[50,"帆布围裙","10支合纱 4*4帆布","条"]
[51,"护脚布","10支合纱 4*4帆布","双"]
[52,"风镜","PC镜片、防紫外线","个"]
[53,"护目镜","树脂镜架、防紫外线","副"]
[54,"防护眼镜","霍尼韦尔100200型防护镜","副"]
[55,"大毛巾","全棉、730*500mm（±5mm）","条",null,null,"单重    g"]
[56,"小毛巾","纯棉、不掉毛、730x340mm（±5mm）","条",null,null,"单重    g"]
[57,"肥皂","透明皂242g-252g","块"]
[58,"洗衣粉","无磷型、560g/袋","袋"]
[59,"强力洗衣粉","无磷型、20Kg/桶","桶"]
[60,"皂粉","雕牌天然皂粉 1.6kg/袋","袋"]
[61,"普通雨衣","PVC防水材质、分体式","套"]
[62,"工矿雨衣","纳米环保面料、透气内里、分体式","套"]
[63,"耐油雨衣","耐油环保材质、分体式","套"]
[64,"长筒雨靴","全塑胶、筒高约40cm","双"]
[65,"中筒雨靴","全塑胶、筒高约25cm","双"]
[66,"5指防割钢丝手套","材质：不锈钢 防割等级：5级 尺寸：手长：20cm 手宽9.5cm","双"]
[67,"过滤棉","3M 5N11过滤棉 N95级别  3M防毒口罩配套","片"]
[68,"滤毒盒","GB2890-2009双盒 D-A/E-1(3M防毒面具配套）","个"]
["                      报价说明：\n                      1、交货期：     天。        2、运输费用：到货价含运杂费。\n                      3、此报价含    %增值税。    4、付款方式：货到验收合格后付款。\n                      5、报价有效期：      天。\n\n                                                报价单位（盖章）：\n                                                报 价 人（签字）：\n                                                报价时间："]